Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Period \_\_\_\_\_\_\_\_

End Table Plan of Procedure #12

Drawer Guide

1. Get the Pre-Cut Drawer Guide boards from the wood storage room. You will need 1 strip of the ¼” thick, ¾” wide, 15” long boards and 2 strips of the ¾” thick, ¾” wide, 17” long boards.
2. Cut the ¼” thick strip to the length of the bottom of your drawer.
3. Glue and clamp the ¼” thick board to the bottom of your drawer. Be sure to center the board and keep it straight when gluing and clamping. Let it dry for at least 30 min.
4. Cut both ¾” thick boards to the length of the inside of your table from the back to the front of your D-Ring MINUS ¾”.
5. Place both strips on your D-Ring and mark where the edge of the D-Ring hits the boards in front and back.
6. Measure and mark a line ¼” down near both ends of each board.
7. See Picture for how your boards will look.
8. Use the BAND SAW to cut out your marks.
9. Place your two drawer guides in your table making sure they fit into the D-Ring. Do not glue these until you have marked where they will be placed by setting your drawer into your table and squeezing the two drawer guides together until they hit the drawer guide on the bottom of your drawer.
10. Mark where the two drawer guides are now at on your D-Ring to know where these will be glued.
11. Glue and clamp both drawer guides onto the D-Ring making sure to line them up where you marked them. Use the small SPRING CLAMPS for this and let dry for at least 30 min.
12. Teacher Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_